Rivo3 Software Changelog


Rivo 3.5.3

1. Resolved an issue that prevented time synchronization during software updates.
2. Fixed an issue where recording did not work after a factory reset.
3. You can now receive iPhone notifications on Rivo via vibration feedback (requires a one-time connection to the Rivo app to enable this feature).


Rivo 3.5.2

1. Improved battery usage time.
2. In the Recordings folder, improved the experience so you no longer need to press and hold L1 to refresh the file list.
3. On iPhone, you can toggle VoiceOver on/off by holding L1 and quickly pressing R4 three times.
4. Fixed an intermittent update failure issue, and Rivo now provides a spoken confirmation of whether the update was successful.


Rivo 3.5

1. Increased the playback limit in Music, Audiobook, and Recordings from 300 files to about 10× more.
2. Fixed an issue on devices running Android 16 where the star button did not move to the parent item.
3. Improved stability for intermittent disconnections with Android devices in certain environments.


Rivo 3.4.2

1. In supported apps, pressing R3 sends a message and R4 + R3 inserts a line break, or the reverse, depending on the app's settings.


Rivo 3.4.1

1. Minor issues fixed.


Rivo 3.4

1. Minor issues fixed.
2. Adjusted battery level reporting to provide a more consistent and accurate reading.


Rivo 3.3

1. VoiceOver navigation commands have been added as follows:
1.1. R1 + L2 or R2: Move to the previous or next split region on the current screen
1.2. In text mode, R4 + 3: Read the currently selected text

2. TalkBack navigation commands have been added as follows:
2.1. L1 + 0: Move to the Apps folder
2.2. Press and hold L1 + R4: Invoke Bixby on a Galaxy smartphone
2.3. R1 + 0: Open the action menu for the currently selected item

3. You can use a wireless earphone in Rivo Home mode as follows:
3.1. Pair a wireless earphone: Press and hold * + L3
3.2. Connect the wireless earphone: Press * + L3 briefly
3.3. Disconnect the wireless earphone: Press * + R3 briefly
3.4. Remove the wireless earphone: Press and hold * + R3

4. The Rivo software version can be checked in the Rivo Home Help menu.
5. An Audio DAISY Book menu has been added to the Rivo Home menu.


Rivo 3.2.3
1. On Android, 3 or 9 scrolls the screen up or down, and L2 or R2 scrolls left or right.
2. Minor issues fixed.


Rivo 3.2.2

1. To lock or unlock Rivo buttons, press and hold either the KEYBOARD or AUDIO button. There are two vibrations when locked and one vibration when unlocked.
2. To check the date, press the TIME button twice quickly.
3. To check the remaining battery level, press and hold the S1 button.
4. To check the minutes of the current time by vibration, press and hold the S2 button.
5. To answer or end a call, you may also press either the KEYBOARD or AUDIO button twice quickly.
6. Fixed an issue where the back button does not work on some apps in Android.
7. Fixed the Rivo app disconnection issue on the latest Android OS.
8. The initial volume will change to maximum when the Rivo speakerphone is turned on during a call.
9. Fixed an issue where * + L4 and * + R4 did not work for starting and stopping voice recording.
10. Feedback is provided by voice or vibration depending on the settings in Home > Settings > Preferences > Audio Feedback.


Rivo 3.2.1

1. Up to 9 devices from 1 to 9 can be saved and connected conveniently.
2. To search the iPhone screen, press L1 + R1, 7, then change Rivo to a text input mode, enter the search text, and press R3. To search for the previous or next item in the search results, press L1 + R1, 8 or 9.
3. When Rivo is locked, it is unlocked when set to the phone, alarm, or pairing mode.
4. There is only vibration feedback when the audio feedback is off.
5. When entering a date in the Home Calendar menu, press R1 to delete the last input number, and press and hold R1 to delete all the input numbers.
6. When entering braille in the braille dictionary, press and hold R1 to delete all input braille.
7. In the Home Settings menu, press 1 or 7 to jump to the first or last menu.
8. Navigation commands are supported for the Apple Watch.


Rivo 3.2

Initial version for Rivo3S.